Substream2 Settings-HD Encoder

HD Encoder System Platform
Version:

Language（语言）

## Substream2

  Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

Video Codec:

Video Resolutions:

FPS:

Custom FPS:
  [5-30]

GOP:
  [5-300] Group of Pictures, keyframe interval = GOP / FPS

H.264 Level:

Bitrate Control:

Fluctuation Level:

Image Quality:

Bitrate(Kbit):
  [32-32000]

JPG URL:

MJPG URL:

TS URL:

HLS TS URL:

HLS MP4 URL:

MP4 URL:

FLV URL:

RTSP URL:

RTSP Multicast IP:

RTSP Multicast port:
  [1-65535]

RTMP URL:

RTMP(S)/RTSP PUSH URL:

Multicast IP:

Multicast Port:
  [1-65535]

Multicast SAP Name:

SRT Listener URL:

SRT Caller URL:

HLS PUSH URL:

## Stream Parameters

TS Video PID:
  [16-8190]

TS Audio PID:
  [16-8190]

TS Transport Stream ID:
  [1-65535]

TS Original Network ID:
  [1-65535]

TS PMT Start PID:
  [16-7936]

TS Start PID:
  [32-3840]

TS Tables Version:
  [0-31]

TS Service ID:
  [1-65535]

TS Service Name:

TS Provider Name:

Conform to System B (DVB):

TS Null Packet:

TS TDT:

## OSD

### Zone 1

Zone:

Alpha:
  [0-128]

Type:

Position:

Speed:
  [0-30]

X:

Y:

Text:

Font Size:
  [8-72]

Background Color:

Color:
  select color

Logo:

### Zone 2

Zone:

Alpha:
  [0-128]

Type:

Position:

Speed:
  [0-30]

X:

Y:

Text:

Font Size:
  [8-72]

Background Color:

Color:
  select color

Logo:

### Zone 3

Zone:

Alpha:
  [0-128]

Type:

Position:

Speed:
  [0-30]

X:

Y:

Text:

Font Size:
  [8-72]

Background Color:

Color:
  select color

Logo:

### Zone 4

Zone:

Alpha:
  [0-128]

Type:

Position:

Speed:
  [0-30]

X:

Y:

Text:

Font Size:
  [8-72]

Background Color:

Color:
  select color

Logo:

### LOGO

LOGO:
  Please upload PNG pictures less than 500 kByte, the file name is logo1.png\logo2.png\logo3.png\logo4.png.