System Settings-HD Encoder

HD Encoder System Platform
Version:

Language（语言）

## Change password

Old Password:

New Password:

Reconfirm Password:

## Advanced

Device Name:

EDID:

Video Only:
  Encode the video only.

Audio Only:
  Encode the audio only.

No Signal Pic Only:
  Only show the preset no signal picture even with video input.

No Signal:
  Display Picture - show the preset no signal picture.

HLS Segment Duration(s):
  [3-20]

HLS Segment Quantity:
  [3-20]

TS Muxer:

Net Drop Threshold:
  [50-50000]

TS Once Pack:
  [3-128]

TS/RTSP Password Enable:

HTTP No Password:

Telnet Service:

Samba Service:

Onvif Service:

RTSP Default Stream:

vMix Compatible:

TS Over RTSP:

Multicast Type:

Enable SAP:

SLICE Number:
  [1-255]

CBR MIN QP:
  [1-35]

CBR MAX QP:
  (MIN_QP-50]

MTU Size:
  [500-8000]

Ethernet Speed:

UDP TTL:
  [1-254]

UDP SOCKET_BUF_SIZE:
  (0-20971520]

PAR:
  (DAR = SAR x PAR)

Kick All When Input Changed:
  Disconnect all players when audio/video input changes.

No Video Auto Restart:
  If no video is detected, the encoder will automatically reboot after 3 minutes.

No Audio Auto Restart:
  If no audio is detected, the encoder will automatically reboot after 3 minutes.

Screen Freeze Auto Reboot:
  If screen freeze detected, the encoder will automatically reboot after 1 minute.

Deblocking Enable:

Deblocking Alpha:
  [-6~6]

Deblocking Beta:
  [-6~6]

## Serial to TCP

Mode:

Baud Rate:

Server Address:

Server Port:
  [1-65535]

## Schedule Restart

Restart Enable:

Restart Time:

## NTP

NTP Enable:

NTP Server:

Time Zone:

## Upload Firmware and Configuration

Select File:
  (File name must be 'up.rar' or 'box.ini'. Do not upload concurrently or power off during the upgrade process.)

## Backup firmware and configuration

## System Settings