Status Display-HD Encoder

HD Encoder System Platform
Version:

Language（语言）

## Input Status

Running Time:

Device Time: (Sync Time To Device)

Device Name:

CPU Usage:

Memory Usage:

Codec Usage:

Input Resolution:
(VGA automatic adjustment)

Video Status:

Collected Video Frames:

Audio Sample Rate:

Audio Status:

Collected Audio Frames:

Net Status:

Net Packet Sent:

Net Packet Dropped:

Preview(Low Delay)

Advanced Compression:

## Record Status

SD Card Status: unformart

Total Disk Space:

Free Disk Space:

Samba Address:

Record Status:
(Delete All Video Files)

Disk Status: Full

Disk Status: Too Slow

## DHCP Status

IP:

Netmask:

Gateway:

## WIFI Status

WIFI: Disable

WIFI Status:

WIFI SSID:

WIFI IP:

WIFI MAC:

WIFI Level:

WIFI Freq:

## 4G Status

4G: Disable

4G Status:

4G IMEI:

4G Mode:

4G Level:

4G Online:

4G Rx:

4G Tx:

4G IP:

4G Gateway:

## Main Stream

Video Codec:

Video Resolution:

Bitrate(Kbit):

MJPG URL:

JPG URLL:

TS URL:

HLS TS URL:

HLS MP4 URL:

MP4 URL:

FLV URL:

RTSP URL:

RTMP(S) PUSH URL0:

RTMP(S) PUSH URL1:

RTMP(S) PUSH URL2:

Multicast URL:

SRT Listener URL:

SRT Caller URL:

HLS PUSH URL:

ICECAST PUSH URL:

TRTC Room:

Preview(HTML5)

Preview(HTML5)

## Substream1

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

Video Codec:

Video Resolution:

Bitrate(Kbit):

MJPG URL:

JPG URL:

TS URL:

HLS TS URL:

HLS MP4 URL:

MP4 URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP(S) PUSH URL0:

RTMP(S) PUSH URL1:

RTMP(S) PUSH URL2:

Multicast URL:

SRT Listener URL:

SRT Caller URL:

HLS PUSH URL:

ICECAST PUSH URL:

Preview(HTML5)

Preview(HTML5)

## Substream2

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

Video Codec:

Video Resolution:

Bitrate(Kbit):

MJPG URL:

JPG URL:

TS URL:

HLS TS URL:

HLS MP4 URL:

MP4 URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP(S) PUSH URL0:

RTMP(S) PUSH URL1:

RTMP(S) PUSH URL2:

Multicast URL:

SRT Listener URL:

SRT Caller URL:

HLS PUSH URL:

Preview(HTML5)

Preview(HTML5)

## Substream3

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

Video Codec:

Video Resolution:

Bitrate(Kbit):

MJPG URL:

JPG URL:

TS URL:

HLS TS URL:

HLS MP4 URL:

MP4 URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP(S) PUSH URL0:

RTMP(S) PUSH URL1:

RTMP(S) PUSH URL2:

Multicast URL:

SRT Listener URL:

SRT Caller URL:

HLS PUSH URL:

Preview(HTML5)

Preview(HTML5)